//
// Copyright (C) 2018 Christoph Sommer <sommer@ccs-labs.org>
//
// Documentation for these modules is at http://veins.car2x.org/
//
// SPDX-License-Identifier: GPL-2.0-or-later
//
// This program is free software; you can redistribute it and/or modify
// it under the terms of the GNU General Public License as published by
// the Free Software Foundation; either version 2 of the License, or
// (at your option) any later version.
//
// This program is distributed in the hope that it will be useful,
// but WITHOUT ANY WARRANTY; without even the implied warranty of
// MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
// GNU General Public License for more details.
//
// You should have received a copy of the GNU General Public License
// along with this program; if not, write to the Free Software
// Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
//

package org.car2x.veins.subprojects.veins_inet;

import inet.applications.contract.IApp;

simple VeinsInetApplicationBase like IApp
{
    parameters:
        string interfaceTableModule;   // The path to the InterfaceTable module
        string interface = default("wlan0");  // The interface name of where to send packets (via multicast)

        @display("i=block/app");
        @class(veins::VeinsInetApplicationBase);
        @signal[packetSent](type=inet::Packet);
        @signal[packetReceived](type=inet::Packet);
        @statistic[packetReceived](title="packets received"; source=packetReceived; record=count,"sum(packetBytes)","vector(packetBytes)"; interpolationmode=none);
        @statistic[throughput](title="throughput"; unit=bps; source="throughput(packetReceived)"; record=vector);
        @statistic[packetSent](title="packets sent"; source=packetSent; record=count,"sum(packetBytes)","vector(packetBytes)"; interpolationmode=none);
        @statistic[rcvdPkLifetime](title="received packet lifetime"; source="dataAge(packetReceived)"; unit=s; record=stats,vector; interpolationmode=none);
    gates:
        input socketIn @labels(UdpControlInfo/up);
        output socketOut @labels(UdpControlInfo/down);
}
