<?xml version="1.0" ?>
<COMPONENTS>
  <COMPONENT>
    <NAME>ap_nms_IRFU120_19930601</NAME>
    <VENDOR>---</VENDOR>
    <DESCRIPTION>Basic Description: NMOS Transistor, Part number: IRFU120, Key parameters: Vto=3.417 Kp=5.646</DESCRIPTION>
    <LIBRARY>Analog_Parts_Library</LIBRARY>
    <PLACEMENT>Both</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE>
</LICENSE>
  </COMPONENT>
  <COMPONENT>
    <NAME>ap_nms_BS170_19930601</NAME>
    <VENDOR>Motorola</VENDOR>
    <DESCRIPTION>Manufacturer: Motorola, Basic Description: NMOS Transistor, Part number: BS170, Key parameters: Vto=3.8 Kp=9</DESCRIPTION>
    <LIBRARY>Analog_Parts_Library</LIBRARY>
    <PLACEMENT>Both</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE>
</LICENSE>
  </COMPONENT>
  <COMPONENT>
    <NAME>ap_npn_Q2N3904_19930601</NAME>
    <VENDOR>National</VENDOR>
    <DESCRIPTION>Manufacturer: National, Basic Description: NPN Transistor, Part number: Q2N3904, Package: TO-92, Key parameters: Is=6.734e-15 Bf=416.4 Tf=301.2e-12</DESCRIPTION>
    <LIBRARY>Analog_Parts_Library</LIBRARY>
    <PLACEMENT>Both</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE>
</LICENSE>
  </COMPONENT>
  <COMPONENT>
    <NAME>ap_dio_1N4004_19930601</NAME>
    <VENDOR>---</VENDOR>
    <DESCRIPTION>Basic Description: Diode, Part number: 1N4004, Key parameters: Is=5.57515E-10</DESCRIPTION>
    <LIBRARY>Analog_Parts_Library</LIBRARY>
    <PLACEMENT>Both</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE>
</LICENSE>
  </COMPONENT>
  <COMPONENT>
    <NAME>VAR</NAME>
    <VENDOR>N/A</VENDOR>
    <DESCRIPTION>Variables and Equations</DESCRIPTION>
    <LIBRARY>Data Items</LIBRARY>
    <PLACEMENT>NOLAYOUT</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE>
</LICENSE>
  </COMPONENT>
  <COMPONENT>
    <NAME>ap_nms_IRF510_19930601</NAME>
    <VENDOR>International_Rectifier</VENDOR>
    <DESCRIPTION>Manufacturer: International_Rectifier, Basic Description: NMOS Transistor, Part number: IRF510, Key parameters: Vto=3 Kp=2.59155E-05</DESCRIPTION>
    <LIBRARY>Analog_Parts_Library</LIBRARY>
    <PLACEMENT>Both</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE>
</LICENSE>
  </COMPONENT>
  <COMPONENT>
    <NAME>V_DC</NAME>
    <VENDOR>N/A</VENDOR>
    <DESCRIPTION>DC Voltage Source</DESCRIPTION>
    <LIBRARY>Sources-Freq Domain</LIBRARY>
    <PLACEMENT>NOLAYOUT</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE></LICENSE>
  </COMPONENT>
  <COMPONENT>
    <NAME>I_DC</NAME>
    <VENDOR>N/A</VENDOR>
    <DESCRIPTION>DC Current Source</DESCRIPTION>
    <LIBRARY>Sources-Freq Domain</LIBRARY>
    <PLACEMENT>NOLAYOUT</PLACEMENT>
    <AVAILABILITY>Available</AVAILABILITY>
    <URL>N/A</URL>
    <LICENSE>N/A</LICENSE>
  </COMPONENT>
</COMPONENTS>
